**PAPER : SBI clerk Computer knowledge Expected Solved Paper**

**1. A Compiler is \_\_\_\_**(A) A combination of computer hardware  
(B) A program which translates from one high-level language to another  
(C) A program which translates from one high-level to a machine level  
(D)None of these  
Ans : C

**2. When a key is pressed on the keyboard, which standard is used for converting the keystroke into the corresponding bits**(A)ANSI  
(B) ASCII  
(C) EBCDIC  
() ISO  
Ans : A

**3. A Pixel is -**(A) A computer program that draws picture  
(B) A picture stored in secondary memory  
(C) The smallest resolvable part of a picture  
(D) None of these  
Ans : C

**4. Which device is used as the standard pointing device in a Graphical User Environment**(A) Keyboard  
(B) Mouse  
(C) Joystick  
(D) Track ball  
Ans : B

**5. Which number system is usually followed in a typical 32-bit computer?**(A) 2  
(B) 10  
(C) 16  
(D) 32  
Ans : A

**6. Which of the following is not an output device?**(A)Scanner  
(B) Printer  
(C) Flat Screen  
(D) Touch Screen  
Ans : D

**7. Which of the following devices have a limitation that we can only information to it but cannot erase or modify it**(A) Floppy Disk  
(B) Hard Disk  
(C) Tape Drive  
(D) CDROM  
Ans : D

**8. Which technology is used in Compact disks?**(A) Mechanical  
(B) Electrical  
(C) Electro Magnetic  
(D) Laser  
Ans : D

**9. Which of the following storage devices can store maximum amount of data?**(A) Floppy Disk  
(B) Hard Disk  
(C) Compact Disk  
(D) Magneto Optic Disk  
Ans : B

**10. Which of the following is the largest manufacturer of Hard Disk Drives?**(A) IBM  
(B) Segate  
(C) Microsoft  
(D) 3M  
Ans : B

**11. The memory location address are limited to**(A) 00000 to 9ffff(16)  
(B) 00001 to 9ffff(16)  
(C) 00010 to 9ffff(16)  
(D) 10000 to 9ffff(16)  
Ans : A

**12. The programs which are as permanent as hardware and stored in ROM is known as**(A) Hardware  
(B) Software  
(C) Firmware  
(D) ROMware  
Ans : C

**13. Memory is made up of**(A) Set of wires  
(B) Set of circuits  
(C) Large number of cells  
(D) All of these  
Ans : C

**14. Primary memory stores**(A) Data alone  
(B) Programs alone  
(C) Results alone  
(D) All of these  
Ans : D

**15. EPROM can be used for**(A) Erasing the contents of ROM  
(B) Reconstructing the contents of ROM  
(C) Erasing and reconstructing the contents of ROM  
(DS) Duplicating ROM  
Ans : C

**16. Which device can understand difference between data & programs?**(A)Input device  
(B) Output device  
(C) Memory  
(D) Microprocessor  
Ans : D

**17. The contents of information are stored in**(A) Memory data register  
(B) Memory address register  
(C) Memory access register  
(D) Memory arithmetic register  
Ans : A

**18. Memory unit is one part of**(A) Input device  
(B) Control unit  
(C) Output device  
(D) Central Processing Unit  
Ans : D

**19. Algorithm and Flow chart help us to**(A) Know the memory capacity  
(B) Identify the base of a number system  
(C) Direct the output to a printer  
(D) Specify the problem completely and clearly  
Ans : D

**20. Which of the following is not a valid size of a Floppy Disk?**(A) 8"  
(B) 5 1/4"  
(C) 3 1/2"  
(D) 5 1/2"  
Ans : B