**PAPER : SBI clerk Computer knowledge Expected Solved Paper**

**1. A Compiler is \_\_\_\_**(A) A combination of computer hardware
(B) A program which translates from one high-level language to another
(C) A program which translates from one high-level to a machine level
(D)None of these
Ans : C

**2. When a key is pressed on the keyboard, which standard is used for converting the keystroke into the corresponding bits**(A)ANSI
(B) ASCII
(C) EBCDIC
() ISO
Ans : A

**3. A Pixel is -**(A) A computer program that draws picture
(B) A picture stored in secondary memory
(C) The smallest resolvable part of a picture
(D) None of these
Ans : C

**4. Which device is used as the standard pointing device in a Graphical User Environment**(A) Keyboard
(B) Mouse
(C) Joystick
(D) Track ball
Ans : B

**5. Which number system is usually followed in a typical 32-bit computer?**(A) 2
(B) 10
(C) 16
(D) 32
Ans : A

**6. Which of the following is not an output device?**(A)Scanner
(B) Printer
(C) Flat Screen
(D) Touch Screen
Ans : D

**7. Which of the following devices have a limitation that we can only information to it but cannot erase or modify it**(A) Floppy Disk
(B) Hard Disk
(C) Tape Drive
(D) CDROM
Ans : D

**8. Which technology is used in Compact disks?**(A) Mechanical
(B) Electrical
(C) Electro Magnetic
(D) Laser
Ans : D

**9. Which of the following storage devices can store maximum amount of data?**(A) Floppy Disk
(B) Hard Disk
(C) Compact Disk
(D) Magneto Optic Disk
Ans : B

**10. Which of the following is the largest manufacturer of Hard Disk Drives?**(A) IBM
(B) Segate
(C) Microsoft
(D) 3M
Ans : B

**11. The memory location address are limited to**(A) 00000 to 9ffff(16)
(B) 00001 to 9ffff(16)
(C) 00010 to 9ffff(16)
(D) 10000 to 9ffff(16)
Ans : A

**12. The programs which are as permanent as hardware and stored in ROM is known as**(A) Hardware
(B) Software
(C) Firmware
(D) ROMware
Ans : C

**13. Memory is made up of**(A) Set of wires
(B) Set of circuits
(C) Large number of cells
(D) All of these
Ans : C

**14. Primary memory stores**(A) Data alone
(B) Programs alone
(C) Results alone
(D) All of these
Ans : D

**15. EPROM can be used for**(A) Erasing the contents of ROM
(B) Reconstructing the contents of ROM
(C) Erasing and reconstructing the contents of ROM
(DS) Duplicating ROM
Ans : C

**16. Which device can understand difference between data & programs?**(A)Input device
(B) Output device
(C) Memory
(D) Microprocessor
Ans : D

**17. The contents of information are stored in**(A) Memory data register
(B) Memory address register
(C) Memory access register
(D) Memory arithmetic register
Ans : A

**18. Memory unit is one part of**(A) Input device
(B) Control unit
(C) Output device
(D) Central Processing Unit
Ans : D

**19. Algorithm and Flow chart help us to**(A) Know the memory capacity
(B) Identify the base of a number system
(C) Direct the output to a printer
(D) Specify the problem completely and clearly
Ans : D

**20. Which of the following is not a valid size of a Floppy Disk?**(A) 8"
(B) 5 1/4"
(C) 3 1/2"
(D) 5 1/2"
Ans : B